# Windows 95 Troubleshooting

If you can’t connect to a server or if Windows 95 reports an error after you double-click Network Neighborhood, try the suggestions here first, refer to the general troubleshooting steps if necessary.

- Make sure you’re using the drivers that are on the drivers CD that ships with this adapter.

- Make sure the driver is loaded and the protocols are bound. Check the Device Properties list for trouble indicators (an X or ! symbol).

- Test the adapter with the Intel® PROSet advanced configuration utility that was installed on your system when you installed the PRO/100 S Server adapter. To start Intel PROSet, double-click the Intel PROSet icon in Control Panel. To run diagnostics, select the adapter and click the Diagnostics tab, then click Run Tests. For additional information, click Help in the Intel PROSet window.

- Check with your LAN administrator — you may need to install additional networking software.

`Last modified on 9/18/03 1:08p Revision 1`