# Server System Setup

Overview

Windows* 2000 RIS Server Setup

Linux* Server Setup

Other Server Setup Information

## Overview

For the Intel Boot Agent software to perform its intended job, there must be a server set up on the same network as the client computer. That server must recognize and respond to the PXE, RPL, or BOOTP boot protocols that are used by the Intel Boot Agent software.

The following topics describe the actions you should take to set up various types of servers to work with the Intel Boot Agent. If you have questions concerning the setup of your server system, contact the manufacturer of your server hardware or your server operating system vendor for assistance.

| NOTE: When the Intel Boot Agent software is installed as an upgrade for an earlier version boot ROM, the associated server-side software may not be compatible with the updated Intel Boot Agent. Contact your system administrator to determine if any server updates are necessary.

## Windows* 2000 RIS Server Setup

For information about setting up a Windows 2000 RIS Server:

1. Refer to the information located at http://www.microsoft.com/windows2000.

2. Select Technical Resources on the left-hand channel bar.

3. Select How it Works.

4. Under the Management link, select Remote Operating System Installation.

## Linux* Server Setup

Consult your Linux* vendor for information about setting up the Linux Server.

## Other Server Setup Information

An extensive list of hardware and software manufacturers provide products that support remote boot technology, conforming either to the Wired for Management (WfM) specifications or the PXE /RPL/BOOTP/ DHCP protocols. For information about setting up servers, as well as about other remote boot-related products provided by these manufacturers, select Boot-Related Resources.

`Last modified on 2/01/05 9:07a Revision 1`