# Attach the RJ45 Network Cable

Insert the twisted pair, RJ45 network cable as shown.

Use one of the following types of network cabling, depending on your adapter and the intended use: For 1000 Mbps operation (1000BaseT), use Category 5 or better (must be 4-pair wiring). Make sure you use Category 5 cable that complies with the TIA-568 wiring specification. For more information on this specification, see the Telecommunications Industry Association's web site: www.tiaonline.org. For 100 Mbps operation (100BaseTX), use Category 5 wiring or better. For 10 Mbps operation (10BaseT), use Category 3 wiring or better.
| Caution: If using less than 4-pair cabling, you must manually configure the speed and duplex setting of the adapter and the link partner. In addition, with 2- and 3-pair cabling the adapter can only achieve speeds of up to 100Mbps.
If you are using this adapter in a residential environment (at any speed), use Category 5 or better wiring. If the cable runs between rooms or through walls and/or ceilings, it should be plenum-rated for fire safety. In all cases: Segment length is limited to 100 meters. The adapter must be connected to a compatible link partner, and may be set to auto-negotiate speed and duplex. Intel® PRO/1000 Adapters using copper connections automatically accommodate either MDI or MDI-X connections. The auto-MDI-X feature of Intel PRO/1000 copper adapters allows you to directly connect two adapters without using a cross-over cable. | Single-port models Dual-port models

| NOTE: Multi port adapters have multiple Ethernet addresses. The address for the first port (port A or 1) is printed on a label on the component side of the adapter. Add one (hexadecimal) to this address to obtain the value for the second port (port B or 2). For example, if the address on the label is 0002B3002B50, then the second port address is 0002B3002B51.

`Last modified on 11/26/03 4:11p Revision 1`