# Teaming

Teaming is a feature of Intel Advanced Network Services (ANS) software. This is available when two or more suitable adapters are configured to operate as a team using Intel® PROSet software.

## Setting up Adapter Teaming

| IMPORTANT: Be sure to use the latest available drivers on all adapters. If you are using an Intel® PRO/10GbE Server Adapter and an Intel PRO/1000 adapter in the same machine, the driver for the PRO/1000 adapter must be updated with in the version on the Intel PRO/10GbE CD or respective download package. Before creating a team, adding or removing team members, or changing advanced settings of a team member, make sure each team member has been configured similarly. Settings to check include VLANs and QoS Packet Tagging, Jumbo Frames, and the various offloads. These settings are available on the Advanced Settings tab. Pay particular attention when using different adapter models or adapter versions, as adapter capabilities vary. If team members implement Intel ANS features differently, failover and team functionality may be affected. To avoid team implementation issues: Create teams that use similar adapter types and models. Reload the team after adding an adapter or changing any Advanced features. One way to reload the team is to select a new preferred primary adapter. Although there will be a temporary loss of network connectivity as the team reconfigures, the team will maintain its network addressing schema.

| NOTES: Intel PRO/10GbE Server Adapters can team with Intel PRO/1000 adapters and certain server-oriented models from other manufacturers. If you are using a Windows-based computer, adapters that appear in Intel® PROSet may be included in a team. Teaming options are supported on Intel PRO/10GbE and PRO/1000 adapters if there is at least one server adapter installed. Selected adapters from other manufacturers are also supported. If you are using a Windows-based computer, adapters that appear in Intel PROSet may be included in a team. Hot Add/Remove of an adapter to/from a team or VLAN is available in Windows 2000 and Windows Server 2003.

## Adapter Fault Tolerance

Adapter Fault Tolerance (AFT) provides the safety of an additional backup link between the server and switch. In the case of switch port, cable, or adapter failure, you can maintain network connectivity. If the primary adapter fails, the secondary adapter takes over. AFT supports two to eight adapters per team. This teaming mode works with any hub or switch, and all team members must be connected to the same device.

To use Adapter Fault Tolerance, you must have at least one Intel PRO/1000 or PRO/10GbE server adapter in your team. Furthermore, all adapters must be linked to the same switch or hub.

| IMPORTANT: For optimal AFT performance, Spanning Tree Protocol (STP) must be disabled.

### Primary and Secondary Adapters

Adapter Fault Tolerance is implemented with a primary adapter, and one or more backup, or secondary adapters. During normal operation, the primary adapter is the only adapter in the team that responds to traffic. The backup adapters are in standby mode. If the link to the primary adapter fails, the link to the designated secondary adapter automatically takes over.

There are two types of primary and secondary adapters:

- Default primary adapter: If you do not specify a preferred primary adapter, the software will choose an adapter of the highest capability (model and speed) to act as the default primary. If a failover occurs, another adapter becomes the primary. Once the problem with the original primary is resolved, the traffic will not automatically restore to the default (original) primary adapter in most modes. The adapter will, however, rejoin the team as a non-primary.

- Preferred Primary/Secondary adapters: You can specify a preferred adapter in Intel PROSet. Under normal conditions, the Primary adapter handles all traffic. The Secondary adapter will receive fallback traffic if the primary fails. If the Preferred Primary adapter fails, but is later restored to an active status, control is automatically switched back to the Preferred Primary adapter.

To specify a preferred primary or secondary adapter

1. From Device Manager, open the properties of a team.

2. Click the Settings tab.

3. Click the Modify Team button.

4. Select the adapter you want to be the primary adapter and click the Set Primary button.

The adapter's preferred setting appears in the Priority column.

## Switch Fault Tolerance

Switch Fault Tolerance (SFT) teaming allows you to connect each of two teamed adapters to a separate switch.

Switch Fault Tolerance can detect failures when they occur:

- On either teamed adapter

- On either cable connecting the teamed adapter to its switch

- On switch ports connected to the adapters, if link is lost

In SFT teams, one adapter is the primary adapter and one adapter is the secondary adapter. During normal operation, the secondary adapter is in standby mode. In standby, the adapter is inactive and waiting for failover to occur. It does not transmit or receive other network traffic. If the primary adapter loses connectivity, the secondary adapter automatically takes over.

In SFT mode, each adapter in the team can operate at a different speed than the other.

## Multi-Vendor Teaming

Multi-Vendor Teaming (MVT) allows teaming with a combination of Intel and non-Intel adapters. If you are using a Windows-based computer, you can team adapters that appear in Intel® PROSet.

This feature is currently available under Linux, Windows 2000 and Windows Server 2003.

If you are using a Windows-based computer, adapters that appear in Intel® PROSet can be included in a team.

### MVT Design Considerations

- All members in a MVT must operate on a common feature set (lowest common denominator). To assure a common feature set, some advanced features, including hardware offloading, are automatically disabled when non-Intel adapters are team members.

- In order to activate MVT, you must have at least one Intel server adapter in the team, which must be designated as the primary adapter.

- A multi-vendor team can be created for any team mode, but not for VLANs.

- Hot-adding non-Intel adapters to a team causes system instability. For this reason it is recommended that you restart the system or reload the team after hot-adding a non-Intel adapter to a team.

- You must manually verify that the frame setting for the non-Intel adapter matches that of the Intel adapters.

`Last modified on 3/21/05 3:53p Revision 2`