# PCI Hot Plug Support for Microsoft* Windows NT* 4.0

Intel® PRO/100 and Intel® PRO/1000 network adapters are enabled for use in selected servers equipped with PCI Hot Plug support and running Microsoft* Windows NT* 4.0.

| NOTES: If you replace an adapter in a PCI Hot Plug slot, do not place the removed adapter back into the same network until the server has rebooted. The two adapters may have the same Virtual MAC address and create a conflict. PCI Hot Plug will only work when you hot plug an identical Intel network adapter.

For more information on setting up and using PCI Hot Plug support in your server, see your server's documentation.

## Using Hot Plug

To use Hot Plug on Windows NT 4.0 systems, you must install the Intel DMI 2.0 Service Provider. See the Desktop Management Interface (DMI) and Windows Management Instrumentation (WMI) documentation sections for installation and configuration information.

To install an adapter using the Hot Plug feature in Windows NT 4.0 on servers using IBM's Hot Plug, you must first replace the OEMSETUP.INF file in the root directory of your install media with the corresponding file in the \PRO100\WINNT4 or the \PRO1000\WINNT4 directory of the Intel CD. For example, use the MAKEDISK utility to create a Windows NT 4.0 driver diskette. Replace the OEMSETUP.INF file on the driver diskette with the corresponding file in the \PRO100\WINNT4 or the \PRO1000\WINNT4 directory on the Intel CD.

| NOTE: On some systems, replacing the OEMSETUP.INF file will cause a short delay while an adapter team is reset.

`Last modified on 12/06/04 3:46p Revision 1`