## Connect the 10GbE Network Cable

| CAUTION: This product uses a Class 1M laser module. Viewing the laser output with certain optical instruments designed for use at a distance (for example, telescopes and binoculars) may pose an eye hazard.

Remove and save the fiber optic connector cover. Insert a fiber optic cable into the ports on the network adapter bracket as shown.

Most connectors and ports are keyed for proper orientation. If the cable you are using is not keyed, check to be sure the connector is oriented properly (transmit port connected to receive port on the link partner, and vice versa).

For Intel® PRO/10GbE LR Server Adapters: Laser wavelength: 1310 nanometer (not visible). Cable type to use: Single-mode fiber with 9.0mm core diameter Connector type: LC. Maximum cable length: 10 kilometers. For Intel® PRO/10GbE SR Server Adapters: Laser wavelength: 850 nanometer (not visible). Cable type to use: Multi-mode fiber with 62.5mm or 50mm core diameter Connector type: LC or SC. Maximum cable length: 300 meters. The adapter must be connected to a compatible link partner, such as an IEEE 802.3ae-compliant 10-gigabit switch, which is operating at the same laser wavelength as the adapter. Conversion cables to other connector types (such as SC-to-LC) may be used if the cabling matches the optical specifications of the adapter, including length limitations. |

`Last modified on 10/08/04 1:47p Revision 1`