# Remote Wake-Up and Wake on LAN*

## Microsoft* Windows* Products

Microsoft* Windows NT* and Microsoft Windows* 95 are not ACPI-capable. Some settings are not available in these operating systems.

Microsoft Windows 98, Windows Me, Windows 2000, Windows XP, and Windows Server* 2003 are ACPI-capable. These operating systems do not support wake from S5 state, only from standby. When shutting down the system, they shutdown ACPI devices including the Intel PRO adapters. This disarms the adapters remote wake up capability. However, in some ACPI-capable computers, the BIOS may have a setting that allows you to override the OS and wake from an S5 state anyway. If there is no support for wake from S5 state in your BIOS settings, you are limited to Wake From Standby when using these operating systems in ACPI computers.

For some adapters, the advanced tab in Intel® PROSet includes a setting called Enable PME. To explicitly allow wake up with a Magic Packet from shutdown under APM power management mode, set this to Enable.

In ACPI-capable versions of Windows, the Intel PROSet advanced settings also include a setting called Wake on Settings. This controls the type of packets that wake up the system from standby.

In ACPI computers running ACPI-aware operating systems, make sure the wake on standby option is enabled. To enable wake on standby, open the Device Manager and then navigate to the adapter properties Power Management tab. Check the setting “Allow this device to bring the computer out of standby”.

`Last modified on 12/09/04 3:56p Revision 1`