# Performance and Troubleshooting

- PCI Bus Performance Issues

- Common Problems and Solutions

- Multiple Adapters

- PCI and PCI-X Configuration Configuration Troubleshooting

- Other Performance Issues

## PCI Bus Performance Issues

- The entire bus will operate at the speed of the slowest PCI card installed in the bus.

## Common Problems and Solutions

In addition to the table below, review the product release notes.

Problem | Solution
Your computer cannot find the adapter | Make sure the adapter is seated firmly in the slot. Download the latest drivers from the Intel support web site: http://www.intel.com/network Try a different PCI bus master slot. Check to see if your motherboard has the latest BIOS. Make sure your PCI slots are v2.2 compatible. Try rebooting the computer. Try a different Intel adapter.
Diagnostics pass but the connection fails | Check the responding link partner. Make sure the cable is securely attached, is the proper type and does not exceed the recommended lengths. Try another cable. Try running the Sender-Responder diagnostic Test. Make sure the duplex mode and speed setting on the adapter matches the setting on the switch.
Another adapter stops working after you installed the Intel® PRO/1000 adapter | Make sure the cable connections are correct. Make sure your PCI BIOS is current. See PCI Installation Tips. Check for interrupt conflicts and sharing problems. Make sure the other adapter supports shared interrupts. Also, make sure your operating system supports shared interrupts. Unload all PCI device drivers, then reload all drivers. Try reseating all adapters.
Adapter unable to connect to switch at 1000 Mbps, instead connects at 100 Mbps | This is applicable only to copper-based connections. Try another cable. Make sure the adapter and the link partner are set to auto-negotiate. Verify that switch is IEEE 802.3ad-compliant (gigabit over copper) and that you are running the latest operating system revision for your switch.
The adapter stops working without apparent cause | The network driver files may be damaged or deleted. Reinstall the drivers. Try reseating the adapter in its slot or different slot, if necessary. Try rebooting the computer. Try another cable. Try a different adapter. Run the adapter and network tests described under "Test the Adapter".
The Link indicator light is off | Check all connections at the adapter and the switch. Run the adapter and network tests described under "Test the Adapter". Make sure you loaded the adapter driver. Try another port on the switch. Make sure the cable is securely attached. Also make sure that it is the proper type and does not exceed the recommended lengths. Make sure that the link partner is configured to auto-negotiate (or forced to match adapter). Verify that the switch is IEEE 802.3ad-compliant.
The link light is on, but communications are not properly established | Make sure the proper (and latest) driver is loaded. Both the adapter and its link partner must be set to either auto-detect or manually set to the same speed and duplex settings.
| NOTE: The adapter's link indicator light may be on even if communications between the adapter and its link partner have not been properly established. Technically, the link indicator light represents the presence of a carrier signal but not necessarily the ability to properly communicate with a link partner. This is expected behavior and is consistent with IEEE's specification for physical layer operation.
RX or TX light is off | Make sure you've loaded the network drivers. Network may be idle; try creating traffic while monitoring the lights. Try another adapter.
The diagnostic utility reports the adapter is "Not enabled by BIOS" | The PCI BIOS isn't configuring the adapter correctly. Try PCI Installation Tips. Try another PCI slot.
The computer hangs when the drivers are loaded | Try changing the PCI BIOS interrupt settings. See PCI Installation Tips.
Event viewer message: A device attached to the system is not functioning | If there is a BIOS setting for "Plug and Play OS", it should be set to "NO" for all versions of Microsoft* Windows*.
Install prompting for Prodd.vxd and Prokddp.vxd files in Micorosoft Windows* 2000 | If you use the Add/Remove Programs icon in the Windows Control Panel to remove an Intel adapter, and then try to install drivers from a later Product CD, you may see a prompt asking for the following files: "Prodd.vxd" "Prokddp.vxd" Microsoft Windows is attempting to install the files associated with the earlier driver, which are not present on the later Product CD. To resolve this problem, finish the installation and choose "Skip" when prompted for a missing file. Instead of removing the driver, update it with the later Product CD. For instructions on updating the adapter driver, see the "Install the Network Drivers" section in this online guide.
Microsoft Windows XP or Microsoft Windows Server* 2003 gives an error "Device cannot start (CODE 10)" when you install or update drivers for your gigabit adapter. | Microsoft Windows XP and Microsoft Windows Server 2003 ship with some older plug-and-play drivers for gigabit adapters present. Because XP has trouble replacing a driver file automatically, updating these drivers with Intel's latest drivers may cause this error message. Rebooting your computer will clear the error and allow you to use the full functionality of your adapter. Disable then enable the adapter in Windows Device Manager.
After upgrading operating systems, Intel® PROSet is no longer available | If you are upgrading a Microsoft Windows operating system and you have Intel PROSet software installed, it will be deleted in the process. You will need to reinstall Intel PROSet.
Terminal Server support | When using Terminal Server, make sure only one session of Intel PROSet is open at any one time. Simultaneous sessions are not supported in Intel PROSet.
The IPv6 protocol does not seem to work after updating adapter drivers on Microsoft Windows 2000 Advanced Servers. | When using Microsoft Windows 2000 Advanced Server SP1 with IPv6 bound to the adapter, you must unbind the IPv6 protocol from the adapter before updating drivers. This is a result of the operating system implementation of the IPv6 protocol. To update an adapter using the IPv6 protocol: Unbind the IPv6 protocol from the adapter. To find the IPv6 setting, click Start > Settings > Control Panel > Network and Dial-Up connections > Local Area Connection <#>, where <#> is the connection number. Right-click the Connection number to open the Adapter Properties dialog box. Clear the IPv6 checkbox then click OK. Update drivers. Bind the IPv6 protocol to the adapter. In the Adapter Properties dialog box, click the IPv6 checkbox. See step one for detailed instructions on finding the IPv6 option.

### Other Items to Check

- Use the drivers that came with your adapter or download the latest drivers from the support website.

- Make sure the cable is installed properly. The network cable must be securely attached at all connections. If the cable is attached but the problem persists, try a different cable.

  - For copper connections, make sure the cable is a 4-pair Category-5 or better.

- Make sure the link partners match or are set to auto-negotiate.

- Test the adapter. Run the adapter and network tests described in Test the Adapter.

- Check the Common problems table and try the recommended solutions.

## Multiple Adapters

When configuring a multi-adapter environment, you must upgrade all Intel adapters in the computer to the latest software.

If the computer has trouble detecting all adapters, consider the following:

- If you enable Wake on LAN* (WoL) on more than two adapters, the Wake on LAN feature may overdraw your system’s auxiliary power supply, resulting in the inability to boot the system and other unpredictable problems. For multiple desktop/management adapters, it is recommended that you install one adapter at a time and use the IBAUtil utility (ibautil.exe in \APPS\BOOTAGNT) to disable the WoL feature on adapters that do not require WoL capabilities. On server adapters, the WoL feature is disabled by default.

- Adapters with Intel Boot Agent enabled will require a portion of the limited start up memory for each adapter enabled. Disable the service on adapters that do not need to boot Preboot Execution Environment (PXE) or Remote Program Load (RPL).

## PCI and PCI-X Configuration Troubleshooting

If the adapter is not recognized by your OS or if it does not work you may need to change some BIOS Setup program settings. Try the following only if you are having problems with the adapter.

- You may need to change the Plug and Play setting in your computer's BIOS. See your computer's manual for instructions on how to access.

- Enable the PCI slot. In some PCI computers, you may need to use the BIOS Setup program to enable the PCI slot.

- You must install the network adapter in a bus master slot. Some BIOS Setup programs require you to enable the slot for bus master/master. Check your BIOS Setup program and the computer's documentation to make sure the slot is set for bus master/master.

- Configure the slot for level-triggered interrupts. The PCI slot the adapter is using must be configured for level-triggered interrupts instead of edge-triggered interrupts. Check your BIOS Setup program to make sure triggering is set up properly.

- Reserve interrupts and/or memory addresses in the BIOS. This prevents PCI cards from trying to use the same settings as ISA cards. Check your BIOS Setup program; there may be IRQ options such as Enable for ISA or Disable for PCI.

Here are some examples of BIOS Setup program parameters:

> PCI slot #: Slot where the adapter is installed
> Master: ENABLED
> Slave: ENABLED
> Latency timer: 40 - 80
> Interrupt: Choose any one of several that the BIOS Setup provides.
> Edge-level: Level

The exact wording of the parameters varies with different computers.

## Other Performance Issues

Attaining gigabit speeds requires that many components are operating at peak efficiency. Among them are the following:

- Cable quality and length. Do not exceed the maximum recommended length for your cable type. Shorter lengths provide better results. Straighten kinks and check for damaged sections of cable.

- Bus speed and traffic

- Processor speed and load

- Available memory

- Transmission frame size (see Jumbo Frames)

- Operating System - Features will vary by OS compatibility, such as offloading and multiprocessor threading.

`Last modified on 12/21/04 2:54p Revision 1`